>>> H81-OPS-I7-4770+8G+128/256/512G Specifications <<<

|  |  |
| --- | --- |
|  |  |
| **C:\Users\Administrator\Desktop\微信图片_20210803162816.jpg微信图片_20210803162816** | **Features:** |
| 1. Front VGA+HDMI port, easy to use. |
| 2. Build in WIFI. |
| 3. Support traditional Intel Core processor. |
| 4. Mainboard supports one key to recover OS. |

|  |  |  |
| --- | --- | --- |
| Processor | Chip | B85 |
| CPU | Intel® Core™ i7-4770 |
| Performance Spec. | # of Cores: 4 # of Threads: 8 Processor Base Frequency: 3.4GHz |
| Memory | Technology | 1 x SODIMMs DDR3 |
| Memory | 8G |
| Display |  Front Output | VGA-Max.1920 x 1080@60hz |
| HDMI-Max. 3840 x 2160@30hz |
| JAE Connector | HDMI-Max. 3840 x 2160@30hz |
| Processor Graphics | Model | Intel® HD Graphics 4600 |
| Base Frequency | 350 MHz |
| Max. Dynamic Frequency | 1.10 GHz |
|  Hard Disk | SSD | 128G or 256G or 512G |
| Network Card | Interface | PCIE |
| Support | 2.4G (5G for option) |
| Gigabit LAN Controller |
| I/O Port | JAE Connector | 1(JAE TX25 80-PIN) |
| VGA | VGA-Max.1920X1080@60hz |
| HDMI | HDMI-Max. 3840 x 2160@30hz |
| LAN | 1(RJ45. Gigabit) |
| USB | 2 x USB3.0 & 4 x USB2.0 |
| AUDIO | 1 x AUDIO OUT & 1 x MIC IN |
| Extension Port | Mini-PCLe(built-in) | 1 x Mini-Pcie |
| 1 x Msata |
| Power | Input voltage | DC-IN 12~19V |
| Physical | Size | 180 x 195 x 42 mm |
| Material | Iron sheet |
|  Heat Dissipation | Dissipation | Pure aluminum dual-ball fan for cooling and temperature control |
|  Environment | Temperature | 0 - 40℃ |
| Humidity | 95% @40℃(Non-condensing) |
|  Software Development Kit | OS | Windows® 7 Windows® 10 |
| Power on automatically | Support, hardware control power-on automatic boot, motherboard jump cap mode. |

**Product Dimension**

