>>> H310-I5-8500+8G+256G Catalog <<<

|  |  |
| --- | --- |
|  |  |
| b6a96c77a864a78693d41894ddaa67a  **Photo** | **Main Spec:** |
| 1. Front VGA+HDMI port, support 4K. |
| 2. WIFI antenna. |
| 3. Front and rear JAE connector for optional. |
| 4. Support Intel® Core™ Processor and Intel® Celeron® Processor G Series. |

|  |  |  |
| --- | --- | --- |
| Processor | Chip | Intel® H310 Express |
| CPU | 8th Intel® Core™ i5-8500 |
| Performance Spec. | # of Cores: 6 # of Threads: 6 Processor Base Frequency: 3.0GHz |
| Memory | Technology | 1 x SODIMMs DDR4 |
| Memory | DDR4-8G |
| Display | Front Output | DP-Max.3840 x 1920 |
| VGA-Max.1920 x 1080 |
| JAE Connector | HDMI-Max. 3840 x 1920 |
| Processor  Graphics | Model | Intel® HD Graphics 630 |
| Max. Memory | 64G |
| Base Frequency | 350 MHz |
| Max. Dynamic Frequency | 1.05 GHz |
| Hard Disk | SSD | 256G |
| Network Adaptor-  Dual Band 5G | Interface | PCIE |
| Support | Dual Band 2.4g/5g |
| Gigabit LAN Controller |
| I/O Port | JAE Connector | 1(JAE TX25 80-PIN) |
| DP | DP-Max.3840 x 1920 (Optional) |
| VGA | VGA-Max.1920X1080 |
| HDMI | HDMI-Max.3840 x 1920 |
| LAN | RJ45. Gigabit |
| USB | 4 x USB3.0 & 2 x USB2.0 |
| AUDIO | 1 x AUDIO OUT + 1 x MIC IN |
| Extension Port | Mini-PCLe  (built-in) | 1 x Mini-Pcie |
| 1 x Msata |
| Power | Input voltage | DC-IN 12~19V |
| Physical | Size | 180 x 195 x 42 mm |
| Material | Metal |
| Heat Dissipation | Dissipation | Copper pipe dual-ball fan for cooling and temperature control |
| Environment | Temperature | 0 - 40℃ |
| Humidity | 95% @40℃(Non-condensing) |
| Software Development Kit | OS | Windows® 7.0, Windows® 8.1, Windows® 10, Linux |